**Wet Field Procedures**

The following procedures should be followed when preparing a wet field for play.

1. Remove standing water from field
   1. For small puddles, use puddle pillows. Let pillows soak up water then wring them out with mop bucket along fence.
   2. For large areas of standing water, use a shop vac to remove. Dig a small hole, place hose in hole and use squeegee to push water into hole. Dump shop vac outside of fence.
2. Once standing water has been removed, add field conditioner or speedy dry to fields. Allow the additives to sit on field for about 10 minutes then rake. Use speedy dry sparingly as it hardens
3. At this point, field should be close to playable. Fields can be raked and dragged with Sandpro.

* **DO NOT SQUEEGEE MUD ONTO OUTFIELD – this takes dirt off the infield and creates a lip**
* **DO NOT** bring Sandpro onto field with standing water
* **DO NOT** add dry dirt to muddy field – this will make field slippery